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Congratulations on your purchase of a new Gorsuch Performance Solutions Lightweight Right

Front Brake Kit!

This option is exclusive to Gorsuch and saves 6 to 8lbs depending on existing RF brake setup. It is

primarily designed for late models that always shut the RF brake off or seldom use it. The .25”

wide blade rotor is not designed for heavy braking or high temperatures. If going to a track

where it is known to use the RF, a standard caliper/rotor is preferred. Simply unbolt the

lightweight caliper/rotor/hardware and re-install standard RF components as needed.

What'’s included (Bill of Material):
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Quantity SKU Description

1 RB-06047 Rotor, direct, solid, 280x6.6, slotted, symmetric, blade, 3.4lbs
1 CB-07085 Caliper, 4-piston, 1.25" square, 0.25" rotor

0.5 PB-04108 Pad 6211 shape, BP28
1 BB-01010 GPS bracket, 11x.25" blade rotor
3 TBD short bolts
4 TBD washers
4 TBD thin washers
1 TBD bracket stiffener
2 TBD GPS aluminum bosses
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Assembly Instructions:

1. Install GPS 11” x .25” blade rotor part # RB-06047
onto the hub

2. Install longer 3/8”-16 x %” long bolt, with washer, into
BB-01010, then onto the top mount of the caliper

3. Install the second BB-01010 to the caliper with the short 3/8”-16 x 1” bolt, with washer,
into the lower caliper mount

4. Install 7/16-20 x 1” long hex bolt into the top
bracket and into the spindle.
Leave loose until all bolts are started.
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5. Install strap bracket onto 3/8” bolt that extends from the caliper mount. Note — the
holes in the strap are different sized in each end.

6. Insert lower 7/16” bolt through the strap and bracket into the spindle
7. Then install a nut on the 3/8” thread that is exposed

8. Check the overall assembly for square-ness and ensure the caliper is centered over the
rotor. The next picture shows the overall assembly mounted onto the spindle.
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9. If needed, shims can be installed in two different locations to shift the caliper in-board or
out-board to center it up:

11. Bleed the brake system like normal
12. Go race and win!
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